TonyPi Setup Notes
Connecting to WiFi (for SSH/SFTP)
1. Open a terminal, run vi wpa_supplicant.conf, and add ssid="wifi_name" and psk="password" (with your actual network name and password)
1. To find the Pi's IP address afterward, run hostname -I
1. Current known IP for the TonyPi: 192.168.1.160
Running the Demo
1. The demo uses the Sony DualShock 4 wireless controller — no USB dongle needed, it's set to autoconnect, so just turn it on
1. Open a terminal, navigate to the desktop, and run ./TonyPi_demo.sh
